**2.1 Three Color ESL image format**

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Version** | **Date** | **Change Description** | **Author** |
| V1.0 | 2018/7/13 | Initial version | Ning |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**C O N F I D E N T I A L**

. **Catalogue**

[1. Purpose 3](#_Toc530931222)

[2. ESL Image Format 3](#_Toc530931223)

[3. Appendix 4](#_Toc530931224)

# Purpose

This article describes the ESL image encoding format, which is used to guide third parties to develop images that are generated by the tag generated by their own programs.

# ESL Image Format

105, 1

106,2

3

4

5

6

…


104

The display of the 2.1-inch electronic label is displayed from right to left and from top to bottom.

The resolution of the 2.1-inch electronic tag is 212\*104, which is equivalent to 22048 pixels. Each pixel adopts three-color display, corresponding to binary 00(black), 01(white) and red(11). If byte encoding is used, it is equivalent to 1 byte and can represent 4 pixels. That is, it can be represented by 22048/4=5512 bytes.

When the cloud initiates an image update to an electronic tag, it needs to send 5512 bytes. Because JSON encoding is used, hexadecimal bytes need to be represented by ASCII, so 1 byte corresponds to 2 ASCII, which is equivalent to a picture corresponding to 5512 \*2 ASCII characters. The following examples illustrate:

Example 1: Need to do the following display




1) The top rightmost column (upper right corner) shows 3 black dots;

2) The bottom right column shows 1 red dot (lower right corner);

3) The top right second column show 1 red dot;

The corresponding code is as follows:



For 2.1 inch three color ESL, one column need 26 bytes (104 pixels).

First column:


* The first byte is 0x01: Corresponding binary digit: 0000 0001, that is, the first 3 pixels are 00,00,00, which is black.
* The last byte is 0x56: Corresponding binary digit:

Second column:

* The first byte is 0x95: Corresponding binary digit:

# Appendix

1. We also attach a file "example.bmp" file in the attachment directory, and we also provide the mqtt message that include image content (example.bin.json).



2. We also attach a file “example.bmpz.json” in the same directory. This file was compression encoding. You can see that the file size is very small. We recommend using compressing encoding json message for 2.1inch three color ESL when sending picture to ESL.